QMS JetScript May Require Printing to EPT

DocumentID: 647654
Revision Date: 29-Feb-96 8:19:23 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Solutions: Some users may need to print to EPT when using the QMS JetScript printer. To do this, select Option 8 for Port and enter EPT as the device or file name. The JetScript software adds the name EPT for sending data to the JetScript board without having to know which LPT number is assigned to the JetScript controller. So whenever in doubt, you can always send data to the JetScript controller via the EPT port. Setting the port to EPT has also been found to correct the error "Device Error 22." *This information is given strictly as a troubleshooting option.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.