Okidata ML 380 - Incorrect Top And Bottom Mar

DocumentID: 638170
Revision Date: 29-Feb-96 3:04:51 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Solutions: The Okidata ML 380 Printer has three paper feed modes. Each mode feeds the paper through differently. 1. Continuous Feed Basic Mode. The paper feeds normally in this mode. 2. Paper Tear Off Mode. In this mode, the printer gives an additional form feed at the end of the print job. This allows you to tear off the continuous feed paper. When the next print job is sent, the printer moves the paper back down into the printer. This sometimes causes the text to print at the very top of the page ignoring the top margin and causing a very large bottom margin. To correct this, you can enter a top text adjustment of down 1". 3. Manual Feed Mode. The printer feeds the paper up one inch in this mode also and prints down to the very last line of the page. To correct this, you can set a top text adjustment of up 1".

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.