Brother Twinriter 6 - Dot-Matrix And Daisy Wh

DocumentID: 645793
Revision Date: 29-Feb-96 8:19:09 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Solutions: A customer using a Brother Twinriter 6 wanted to access both the dot-matrix head and the daisy wheel head. Since the same printer driver is used for both, they were able to do this with the use of fonts. The initial base font in the Brother Twinriter 6 driver is dot-matrix. In order to work with both heads, the user needed only to mark the desired daisy wheel font with an asterisk on the Cartridges/Fonts/Print Wheels list (Shift-F7, S, E, 4, Print Wheel). After marking the wheel, the desired daisy wheel font, as well as the desired dot-matrix fonts can be selected through Ctrl-F8. The print head will rotate between the dot-matrix and daisy wheel heads to print the desired font.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.