Sharp PC 6200 CONFIG.SYS File - Similar To To

DocumentID: 641613
Revision Date: 29-Feb-96 8:18:38 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Solutions: A Sharp PC 6200 laptop computer has a ROM drive similar to Toshiba or a PS/1. To allow reading of the CONFIG.SYS from the hard drive, users must run a program called Install which is built-in. Choices given are: A. C: as ROM drive and D: as hard drive, or B. C: as hard drive and no D: drive. Customers have to choose the latter, C: as hard drive and no D: drive, to allow the machine to boot properly since it will only boot from C: drive, and the only control the user has is whether the hard disk drive is C: or not. If this change is made, any info once on drive D: now appears on drive C: automatically. The Sharp 7000 computer can be set up like this, but WPCorp does not have the 6200 in-house to verify. *This information is given as a troubleshooting option.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.