HP DeskJet - Print To Hardware Port Isn't Fas

DocumentID: 645246
Revision Date: 29-Feb-96 8:19:04 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Symptoms: The customer has Print to Hardware Port set to "yes" for his HP DeskJet. But the print speed didn't change. Solutions: Print to Hardware Port speeds up the capability of sending data to the printer. WordPerfect cannot send the data to the printer quicker than the printer can except it. The HP DeskJet only has a 16K buffer. So WP cannot send the information any faster.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.