B: Drive Not Reading Low Density Diskettes

DocumentID: 608047
Revision Date: 29-Feb-96 1:32:35 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Symptoms: The B: drive will not read low density 3.5" diskettes. It has no problem reading high density disks. Solutions: The customer purchased low density diskettes that came formatted as high density for PS/2 machines. Reformatting those diskettes corrected the problem.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.