XON/XOFF Turned On Does Not Allow Any Keystro

DocumentID: 636796
Revision Date: 29-Feb-96 3:04:23 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Symptoms: A user is unable to perform any keystrokes while a document is being printed to his Diablo 620 printer. He has to wait for the print job to be completely printed before he can type. This started happening when they installed WordPerfect 5.1 and did not happen with WordPerfect 5.0. Solutions: The customer had XON/XOFF set to On in his serial port configuration. After turning this off, the problem went away.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.