Panasonic KX-P1695 - Initial Settings And Pro

DocumentID: 641877
Revision Date: 29-Feb-96 8:18:40 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Solutions: To print the initial settings on the Panasonic KX-P1695 printer, users should hold the function button while turning the printer on. The on-line light will flash. Press the Row button until all three row lights are lit. Press the set button to print the settings, then press the function button to return the printer to normal mode. For Program Mode: 1. While the printer is on, press the Function button. (Both of the first two column lights should be lit. If they are not, press Column until both are flashing, and press Set.) 2. Next, press the Row button. (Again, both of the first two column lights should be lit. If they are not, follow the same steps as above to change them.) 3. Now, make these changes permanent by following these steps: a. Press Row until bottom row light is lit. b. Press Column until the column light is above Macro 1. c. Press Line Feed (LF) button (you will hear two beeps). d. Press Set (you will hear one beep). e. Press Function.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.