Diablo 630 Outdenting Problem

DocumentID: 647493
Revision Date: 29-Feb-96 8:19:22 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Symptoms: The Diablo 630 printer has inconsistent vertical and horizontal spacing, such as the outdenting problem. This is fixed by adding the REPOSITION command under VMI. (See P51_282 for steps). Solutions: In testing, I have found that the Diablo 630 will put in a carriage return command when not asked to do so by WP. This is why we have seen problems with outdenting, and also why the REPOSITION command seems to fix the problem since it forces the printer to remember where it is. If the REPOSITION command does not work, then add [32,8] to Horizontal Motion (HMI). This will correct the outdenting problem, but it will cause underline to not work correctly. The Underline Method must be changed from WP's Underline on Separate Pass to Auto Underline in Same Pass.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.