Graphics Printing Garbage - Check "Print To H

DocumentID: 651376
Revision Date: 29-Feb-96 8:29:06 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Solutions: If a customer receives intermittent garbage or ASCII characters while printing a graphic suggest they check the Print to Hardware Port selection. Having this option set to YES may be the cause of the garbage. To eliminate the unwanted characters, the user may change the option to NO or enter the correct information for the options under Advance Setup. Advance Setup is a selection for Print to Hardware Port (Shift-F7, S, 3, 7). Two questions are asked with this option: 1 - Interrupt Request Level (IRQ) 2 - Base Address *This information is given strictly as a troubleshooting option.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.