Incorrect Alignment Printing A Character Foll

DocumentID: 609854
Revision Date: 29-Feb-96 1:34:25 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Symptoms: Horizontal motion is inaccurate when a user prints a graphically-created character followed by an indent to the Alps P2000 . For example, when a user creates the bullet 4,0 then presses Indent, the line below the Indent code outdents. Solutions: The following steps in the PTR Program will correct this problem: 1. Enter the PTR Program, retrieve the .PRS file, and press Enter on the printer name 2. Move to Vertical Motion and press Enter 3. Move to Relative Vertical Motion and press Enter 4. Move to Move Down and press the Right Arrow key to move to the expression box 5. Move to the end of the line and add a space and the word REPOSITION to the codes that are already there 6. Exit the PTR Program and save the changes How/Why: For some reason this printer is not keeping track of the left margin. The above codes will reset the horizontal motion each time the vertical motion is set. The codes should be placed under Vertical Motion even though they are adjusting the horizontal motion.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.