Tandy DMP 133 Suggested Emulation

DocumentID: 647540
Revision Date: 29-Feb-96 8:19:22 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Solutions: A suggested printer emulation for the Tandy DMP 133 printer is the IBM PC Graphics. When using this driver one will need to set the Tandy DMP 133 in the IBM mode. As far as we can tell and what Tandy indicates the proper dip switch settings for this printer are: 1,2 on; 3-10 off.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.