NetLine ManyLink 3.5 Connects Computers For P

DocumentID: 627601
Revision Date: 29-Feb-96 1:42:17 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Symptoms: The customer is using NetLine ManyLink 3.5 (cable version) to hook up several computers for printer sharing. When the user prints Compose characters or graphics to a remote printer, control codes and ASCII characters appear on the printout. Solutions: NetLine uses serial-to-serial cables to link the computers. The customer found that the transmission speed for the serial ports was set too fast. After dropping the speed that ManyLink was transmitting at, the problem was resolved.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.