Epson FX-80 Not Bolding Draft Or High Quality

DocumentID: 644799
Revision Date: 29-Feb-96 8:19:01 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Symptoms: With the Epson FX-80 driver, the customer is not able to get bold printing in draft or high quality. I went into the PTR program and changed his bold method to the way we had it in 5.0. He was not at his screen so I don't know if that will work or not. Solutions: The Auto Bold code was left out of this driver. 1. Enter PTR, retrieve his ALL file, and Enter the Epson printer. 2. Go to Attribute methods and Enter. 3. Enter Bold and then Enter Auto Bold. 4. Press Enter to get into the expression box for Bold ON and add: [27]"E". 5. Move down to Bold OFF and add: [27]"F". 6. Save and update. This has been fixed and will be on the next 5.1 interim release.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.