HP LaserJet IIISi Sheet Feeder - Not Pulling

DocumentID: 646919
Revision Date: 29-Feb-96 8:19:18 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Symptoms: The customer's HP LaserJet IIISi sheet feeder is pulling from Bin 2 when it should pull from Bin 1. Her paper codes are properly placed. Solutions: The customer was only having this problem when she combined Standard and Letterhead forms in her document, where Letterhead was to pull from Bin 2 and Standard from Bin 1. She had her Letterhead form set to Bin 2, but her Standard form was set for Continuous. After the printer printed the Letterhead page, it continued to print from Bin 2. After she changed the location of her Standard form to Bin 1, her problem was solved. *This information is given strictly as a troubleshooting option.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.