Steps To Put Panasonic KX-P1123 Printer Into

DocumentID: 647210
Revision Date: 29-Feb-96 8:19:20 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Symptoms: What steps do you use to put the Panasonic KX-P1123 or Panasonic KX-P1695 into Program mode (PGM)? This printer is similar to the Panasonic KX-P1124. Solutions: The following steps should be used to change the printer into PGM (program) mode. 1. Turn the printer on. 2. Press the Function key. The top row light and the first two column lights should be on. 3. Press the Row key. This will light the first two row lights. The first two column lights should still be lit. 4. If either of the first two column lights are not lit when performing steps 2-3, press the Column key until they blink, and then press Set. 5. After these are set, press the Row key until the bottom row light is the only one lit. 6. Press the Column key until the light is blinking above Macro1. 7. Press the LF key and two beeps will sound. Press the Function key, turn the printer off and back on. This will place the printer in PGM mode.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.