IBM Quietwriter I (Old EPROM) Problem With Ov

DocumentID: 644953
Revision Date: 29-Feb-96 8:19:02 PM

The information in this document applies to:
WordPerfect® 5.1 for DOS

Problem

Symptoms: When the customer uses bold, the printer does not print an overstrike correctly. Instead, the sentence is printed once and the overstrike is printed over to the right of the first sentence. Underline prints in a similar way, printing underline off to right of the text with a "-1" at the end of the line. The user changed the underline method to "WP Underline On Separate Pass" in the PTR program, and it fixed the problem for underline. Solutions: Using the 06/29/90 Program 1 and 2 and the 04/12/90 printer .ALL file, the user could not duplicate the problem. Development felt that if the problem could not be duplicated on WP's printer (WP has the new EPROM and the customer has the old EPROM) that the customer should update the EPROM for their printer. Customers should be referred to IBM.

Answer:

Details:

Product specifications, packaging, technical support and information (*Specifications*) refer to theUnited States retail English version only. Specifications for other versions may vary. All Specifications, claims, features, representations, and/or comparisons provided are correct to the best of our knowledge of the date of publication, but are subject to change without notice.OUR MAXIMUM AGGREGATE LIABILITY TO YOU AND THAT OF OUR DEALERS AND SUPPLIERS IS LIMITED. IT SHALL NOTEXCEED THE AMOUNT YOU PAID TO ACCESS THE INFORMATION. SEE LEGAL DISCLAIMER.